MySQL Bugs #13523

The SQL statement:
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INSERT INTO P330R_tbl (P330R_VRCTRL, P330R_Region_Cods, P330R_Area_Code, PI30R_Section Letter,
P330R,_Pole_umber, P330R_Spur_sequence_Code, P330R_Pole_Sequence._Code, P330R._Source_CB,

P330R Line_Code, P330R,_Zane, F330R_Substation Name, P33R, Swich Fuse_Ref, PG30R,_Valtage,

P330R Feature_Number, F330R Map_Nomber, P330R._Eastings, P330R._Northings, P330R_Identfier,

P330R Previous_Pole_Number, P330R_Status_of_Pol, P330R_Last_Insp_Patroler, P330R _5_N Last_Update,
P330R Last_Inspection_Date, P330R_Last_Inspection_Tine, P330R_Type_of_Last Insp,

P330R Metfiod_of_Last_Insp, P330R_Last_InspTea, P330R_Inspection.scheduled, P330R_Full InspPatroler,
P330R Full_InspDate._Last, P330R._Ful_Insplob_Ref, P330R Full Insphiext_Dus, P330R._Sfty InspPatroler,
P330R Sty _InspDate_Last, P330R_Sfty Insplob, Ref, P330R_Sfty Insphiext_Due, P330R_Repair_Worklob_Ref,
P330R Tree_Worklob_Ref, PI30R_Reinstmentlob. Ref, P30, Reimpreg_Wkiob_Ref,

P330R Consiructionob_Ref, P330R._Refurbishiintiob_Ref, P330R_5pan_Length, P330R._Mid_pan_Height,
P330R Road_Span_Height, P330R,_Temperature_Measired, P330R_Pole Material, F330R.Year_of_Pole,

P330R Species_Origi, PI3OR_Height_of Pole, P330R_Pole_Size, P330R_Dismeter_of Poi,

P330R Basis_of_Helght, P330R_Helgft_of_Gouge Mark, P330R_Measured_Height, P330R_Xarm_or_Conductor,
P330R Wind_Span, P330R_Orignal Preserv, P330R_Reinforcement_Type, P330R. Other_Damage,

P330R Decay Messured, F330R_Groundine.Circum, P330R,_Excavated, PI30R_Highes:_Point_Decay,

P330R Lowest_Point_Decay, PI3OR_Test_Measure_Height, F330R_Crcum_at_Test_Hoft, P330R_Inmer1,

P330R Outerd, P30R_Inner2, P3A0R_Oterz, P33R _Innerd, F330R _Outer, PEAOR _Inerd, P330R_Outer,
P330R Jnners, P330R OuterS, P330R_Ifmere, P330R_Outeré, P330R_Inner7, P330R_Outer?, P330R_Inners,
P330R Outers, F330R_Residual_Strength, P330R_Sutable_Reinforcert, P330R_Pale_Candin,

P330R Pole_Work_Prifiy, P330R_Original_Condifon, P330R_Original_Friorty, F330R_Year_tst Relmpreqn,
P330R_Treatment_Typet, P330R_Quantity1, P330R _Year_2rd_Relmpregn, P330R_Trestment_Type2,

P330R Quantity?, PI30R_Bandage._Applied, P330R_Pole_Type, P330R_Configuration, P330R_ConstrUction_Type,
P330R_Angle_Link, P330R_Angle_of_Deviation, P330R_Tee_Off Phases, PI30R _Tee_Off Type,

P330R Tee_Off_Phase_Cclour, P330R_Stay_Constructont, P330R,_Stay_Anchoringt, P330R_Number of Stays1,
P330R Stay_Construction2, PI30R_Stay_Anchoring2, P3O _Nuriber_of _stays2, P330R_Stay Attachmt_Helght,
P330R _Stay Spread, PI3OR_Stay_Ange, P33OR_Crossarm_Material, F330R_Crossarm_Sie,

P330R Insulator_Materia, PS30R,_Binder_Type, P330R_Conductor_size, P330R_Conductor_Materisl,

P330R Number_of_Conductors, P330R_Factor_of_Safety, P330R_Fole_Equpment, P330R Surge_Divertor_Matrl
P330R _Transformer_Capacky, PI3OR_ransfoimer_Phases, P330R_Equpment,_L, P330R,_Eauipmert.2,

P330R Equipment_3, P330R_Equipment_4, P330R_Equipment S, P330R_Equipment_6, P330R_Equipment 7,
P330R Equpment S, P330R Land_Usage, PI30R_Land_Ownership, P330R_Suface_Type,
P330R Span Crossingl, P330R_Span_Crossing2, F330R_Span_Crossing3, F330R_Span_Crossingd,

P330R Month_Access_From, P30R,_Month._Access_To, P330R_Attachments, P330R._Earth,_Test_Reading,
P330R Work at_Last_Insp, P330R _Tree_Work Last_Insp, P330R_Other_Comments, P330R_Work_Cormments,
P330R Priorty _of_Work, P330R_Dangerous_Siuation, P330R,_Descrption_Danger, P330R_Tres_Giowth_Rate,
P330R Wayleave_Reqired, PA30R Landowner_Agresable, PG30R_Wiayleave_Agreement,

P330R_Landowne? _Neme, PI30R_Landowner_Address, P330R_Source_Batch) VALUES (s, 03, 5, 'T12, '2/1069),
"05(, 002, GMEL', 101, EH27, ‘OMAGH MAIN ARDSTRAW 33K, ndl, 3, 1341665495, ‘137, 240451,
366250, 30000098, 111065, 4, Rabert Kigore', 167018, {d '1997-01-221, 14153, 3, 1, '999999', 0, Robert
Kigore', {d'1997-01-221}, nul, nul nul, ol nuf, nul, nul, nul, nul nl, nl, 33065, 100, 9.3, nul, 3.7, 1, 62, nul,
9,3, 280, 1, nul, nul, , nul, 1, 0, 0, 2, nul, 0, nul o, rwl, rul, ol ol il ol wl, ol il
il nul, nwl, nul nul, ol , 0, 4, nuf, 1, nul o, 0, 0, nul, ,0,0, 1, 1, 1, nul nul, 1,0,0,0,0, 0,0, 3,0,
nul ol nwl 1,1, 1, 1, 14, 1, 3, nul, 2,6, nul, 0,0, 0,0,0,0,0,0,3,,1,0,0,, 0, 1, 12,0, nul, 1, 1, nul,
il 3, 2, nul, 6, 0, 6, mul ol )

o





produces:
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I\ (008 551 v 50103 e avean e iy 5 s chckhe el tht
Corespond 1 your TS Sear varSnfo the i sy o e et 002, 1T S1o1, EHE73) OMAGH
MAIN ARDSTRAW 33KV, null, 3, '1341665499" at line 1 (state 23000, no 1064)





The error is caused by the ‘069\’ for column P33OR_Spur_Sequence_Code immediately before ‘002’. It requires an additional backslash e.g. ‘069\\’ to be accepted via the ODBC driver, but the above SQL works as shown when submitted via the mysql command line.

